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3.5-inch motherboard, onboard Alder Lake -P series processor
» Intel Alder Lake -P Series Processors
» Supports up to 64GB DDR4 SO-DIMM dual-channel memory, frequency 2133/2666/3200MH z
» Integrated Intel 12th generation Xe LP graphics core
» Support VGA, HDMI, LVDS ( 18/24- bit single or dual channel) or EDP
» Support Intel 10/100/1000Mbit Ethernet, SATA, NVME SSD
» Support USB2.0 and USB3.0 , serial port, GPIO interface
» Input voltage: +12V~+21V , + 12V is recommended
» Operating temperature: -20 °C ~ + 60 °C (optional -40°C ~ + 70 °C ) 
PCM-ADP351 Block Diagram
Single/Dual channel LVDS 24/18
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4x USB3.0



























	Technical Information
	

	Plate Type
	
	3.5 inch motherboard

	Processor
	
	Intel Core ™ i3- 1215U(E),2C+4A,up to 4.4 GHz (P-Core) 3.3 GHz (E-Core),15W-55W
Intel Core ™ i3- 1220P,2C+8A,up to 4.4 GHz (P-Core) 3.3 GHz (E-Core), 28W-64W
Intel Core ™ i 5 - 1235U,2C+8A,up to 4.4 GHz (P-Core) 3.3 GHz (E-Core),15W-55W
Intel Core ™ i 5 - 1240P,4C+8A,up to 4.4 GHz (P-Core) 3.3 GHz (E-Core), 28W-64W
Intel Core™ i5-1245UE,2C+8A,up to 4.4GHz(P-Core) 3.3GHz(E-Core),15W-55W
Intel Core ™ i 7 - 1255U,2C+8A,up to 4.7 GHz (P-Core) 3.5 GHz (E-Core),15W-55W
Intel Core ™ i 7 - 1265U,2C+8A,up to 4.8 GHz (P-Core) 3.6 GHz (E-Core),15W-55W
Intel Core ™ i 7 - 1265UE,2C+8A,up to 4.7 GHz (P-Core) 3.5 GHz (E-Core),15W-55W
Intel Core  i3-1315U (E) ,2C+4A,up to 4. 5 GHz(P-Core) 3.3GHz(E-Core),15W-55W
Intel Core™ i5-1335U,2C+8A,up to 4. 6 GHz(P-Core) 3. 4 GHz(E-Core),15W-55W
Intel Core™ i5-1335UE,2C+8A,up to 4.5GHz(P-Core) 3.3GHz(E-Core),15W-55W
Intel Core™ i7-13 5 5U,2C+8A,up to 5. 0 GHz (P-Core) 3.7GHz(E-Core),15W-55W
Intel Core™ i7-1365UE,2C+8A,up to 4.9GHz(P-Core) 3.7GHz(E-Core),15W-55W

	Memory
	
	Two dual-channel SO-DIMM DDR4 memory, maximum 64G, frequency 2133/2666/3200MH z

	Graphics Processing
	
	Supports 1 HDMI with a maximum resolution of 3840x2160 @ 60 Hz and 1 VGA with a maximum resolution of 1920x1080 @ 60Hz.
Supports 1 18/24- bit single-channel or dual-channel LVDS, with a maximum resolution of 1920x1080 @60Hz

	Network Card
	
	Supports 2 Intel 10/100/1000Mbit Ethernet ( Intel ® I219V and I211AT/I210AT )

	Storage
	
	Supports 1 SATA 3.0 interface, 1 M.2 SSD ( M-Key 2280 SSD Nvme )

	mPCIe
	
	Support 1 M.2 WIFI ( E-Key 2230 PCIe x1 & USB2.0 )
Supports 1 M.2 4G/5G ( B-Key 3042 /3052 USB2.0 & PCIe x1 )

	USB
	
	Support 4 USB3.0/2.0 (front), 4 USB2.0 (built-in)

	Serial Port
	
	Support 6 RS232 (3-wire), COM1 and COM2 can select RS232/422/485

	IO
	
	Supports 8 GPIOs, 1 SIM card slot (expandable, optional)

	Sound Card
	
	ALC662 /ALC897 high-fidelity sound card ( Line-in, Line-out, Mic-in )

	Power Supply
	
	+12V~+21 V , + 12V is recommended

	Temperature
	
	Operating temperature -20°C ~ + 60 °C (optional -40°C ~ + 70 °C )

	Size
	
	146 mm x 10 2 mm

	Heat Dissipation
	
	Fan cooling

	[bookmark: _GoBack]Operating System
	
	Win10, Win11, Linux
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