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3.5-inch motherboard, onboard TIGER LAKE U series processor
» Intel Tiger Lake U series processors
» Supports up to 32GB DDR4 SO-DIMM dual-channel memory, frequency 2133/2666/3200MH z
» Integrated Intel 12th generation Xe LP graphics core
» Support VGA, HDMI, LVDS ( 18/24- bit single or dual channel) or EDP
» Support Intel 10/100/1000Mbit Ethernet, SATA, NVME SSD
» Support USB2.0 and USB3.0 , serial port, GPIO interface
» Input voltage: +12V~+21V , + 12V is recommended
» Operating temperature: -20°C ~ + 60 °C (optional -40°C ~ + 75 °C) 
PCM -T351 Block Diagram
Single/Dual channel LVDS 24/18
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	Technical Information
	

	Plate Type
	
	3.5 inch motherboard

	Processor
	
	Intel Core ™ i3- 1115G4,2C4T,up to 4.1 GHz
Intel Core ™ i3- 1125G4,4C8T,up to 3.7 GHz
Intel Core ™ i 5 - 1135G7,4C8T,up to 4.2 GHz
Intel Core ™ i 5 - 1145G7,4C8T,up to 4.4 GHz
Intel Core ™ i 7 - 1165G7,4C8T,up to 4.7 GHz
Intel Celeron 6305,2C2T,1.8 GHz
Intel Celeron 6305E,2C2T,1.8 GHz

	Memory
	
	Two dual-channel SO-DIMM DDR4 memory, maximum 32G, frequency 2133/2666/3200MH z

	Graphics Processing
	
	Supports 1 HDMI with a maximum resolution of 3840x2160 @ 60 Hz and 1 VGA with a maximum resolution of 1920x1080 @ 60Hz.
Supports one 18/24- bit single-channel or dual-channel LVDS

	Network Card
	
	Support 2 Intel 10/100/1000Mbit Ethernet ( Intel ® I219V /LM and I211AT/I210AT )

	SATA
	
	Supports 1 SATA 3.0 interface, 1 M.2 SSD ( M-Key 2280 SSD Nvme )

	mPCIe
	
	Support 1 M.2 WIFI ( E-Key 2230 PCIe x1 )
Supports 1 M.2 4G/5G ( B-Key 3042 /3052 USB2.0 & PCIe x1 )

	USB
	
	Support 4 USB3.0/2.0 (front), 4 USB2.0 (built-in)

	Serial Port
	
	Support 6 RS232 (3-wire), COM1 and COM2 can select RS232/422/485

	IO
	
	Supports 8 GPIOs, 1 SIM card slot (expandable, optional)

	Sound Card
	
	ALC662 high-fidelity sound card ( Line-in, Line-out, Mic -in )

	Power Supply
	
	+12V~+21 V , + 12V is recommended

	Temperature
	
	Operating temperature -20°C ~ + 60 °C (optional -40°C ~ + 75 °C )

	Size
	
	146 mm x 10 2 mm

	Heat Dissipation
	
	Fan cooling

	[bookmark: _GoBack]Operating System
	
	Win10, Win11, Linux
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