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Intelligent Vehicle Controller
) (
The VIC-RB-04 is a high-performance, highly integrated and reliable
) (
vehicle controller supporting CAN, Gigabit Ethernet, Fast Ethernet
) (
and AHD video input. Provision is made for RS232, RS485, HDMI,
) (
mSATA SSD storage and TF card storage.
) (
Product Features
) (
Technical Specifications
) (
Hardware
) (
Processor
) (
RK3588J ARM Cortex-A76 (4 cores) + Cortex-A55 (4 cores)
) (
Clock Speed
) (
AI Performance
) (
8K P60 H.264/H.265 decoding
) (
Memory
) (
Storage
) (
8K P30 H.264/H.265 encoding
) (
Video Encoding
) (
Video Decoding
) (
Watchdog
) (
Supported
) (
Supported
) (
HDMI + AHD video output
) (
Up to 8K@60fps
) (
Software
) (
Operating System
) (
2 Gigabit Ethernet ports
) (
2 Fast Ethernet ports
) (
RKNN-Toolkit offers easy-to-use, one-click model conversion for
) (
Caffe / TensorFlow / TF-Lite / ONNX / PyTorch / Keras / Darknet models.
) (
Compact, highly integrated design
) (
External Interfaces
) (
Desktop or wall mounting
) (
4 AHD channels supported
) (
Video Output
) (
IP65 protection
) (
Ethernet
) (
2 x Gigabit Ethernet (M12 X-coded, 8-pin), independent ports
) (
2 x Fast Ethernet (M12 D-coded, 4-pin), switched ports
) (
Low power consumption
) (
Serial Ports
) (
1 x RS485, 1 x RS232, 1 x Debug (RS-232)
) (
Efficient passive enclosure cooling for reliable operation
) (
SIM Card
) (
1 x standard SIM card slot
) (
Antennas
) (
2 x GNSS antenna ports; optional SMA ports for Wi-Fi and 5G/4G antennas
) (
Dimensions
) (
Internal Expansion
) (
1 x miniPCIe: optional mSATA SSD or Wi-Fi module (choose one)
) (
1 x M.2 2242: optional 4G/5G module
) (
Power
) (
Input Voltage
) (
Power Draw
) (
Power-loss Protection
) (
Supported
) (
General Specifications
) (
Dimensions
) (
Weight
) (
Mounting
) (
Wall mounting
) (
Cooling
) (
Natural convection
) (
Environment and Reliability
) (
Operating Temp.
) (
Storage Temp.
) (
Relative Humidity
) (
5% to 95% (non-condensing)
) (
IP Rating
) (
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) (
AI performance: 6 TOPS (INT8)
) (
Units: mm
) (
Ordering Information
) (
Model
) (
Memory
) (
Storage
) (
Contact the manufacturer for other configurations and functions.
) (
Deep Learning
) (
-40°C to 85°C
)
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Interface Diagram
) (
DIP switch 1: enter download mode
) (
DIP switch 2: disable watchdog
) (
2 x Gigabit Ethernet
) (
2 x Fast Ethernet
) (
Optional Accessories
) (
Accessory
) (
Qty.
) (
Specification
) (
Automotive connector cable harness
) (
CAN M12 to flying-lead cable
) (
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VIC-RB-04

FEATURES SPECS
2.0GHz 6TOPS@INT8
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